**Genetic Switches between two population with regards to mRNA and proteins**

**1Qin He, 2 Rubin Wang, 3 Xiaochuan Pan**

1Qin He, East China University of Science and Technology, Meilong 130

2Rubin Wang, East China University of Science and Technology , College address

Email: 1Author’s email id, 2Co-Author’s email id

Contact: 1Author’s contact no., 2Co-Author’s contact no.

**Abstract:**. It is not until the advantage of quantum computing devices, the possibility to store more states than either 0 or 1 in one qubits, bring the wide variety of formation processing tasks that the computation power makes breakthrough in the new era of information process. The noisy intermediate-scale quantum (NISQ) devices are defined as the quantum computer for which general-purpose quantum error correction is not feasible and ineradicable hardware errors with two-qubit operations of proper size in the classification problem of EEG signals. Meanwhile, the Gaussian boson sampling (GBS) has demonstrated to be capable of providing a highly-efficient approach to large-scale implementations limiting the fast gates operations. Furthermore, with the Variational Quantum Eigensolver (VQE) equipped, the hybrid algorithms are realized with available circuit depth in quantum phase estimation, optimizing through operation minimization, with the truth that Bayesian variance methods converge faster than the Bayesian inference methods. Last but not the least, EEG data is usually with noise and to thus to make sure of getting correct results, our model is based on NISQ devices and the correspondent results are analyzed on basis of noisy signals classified by the hybrid system composed of single qubits and 1 classical bit. And the Bose-Einstein condensates, as the experiment well known for its possibility to create observable data of the entangled states, investigating the advantage of combining both quantum and classical bits operations based on many-particle entanglement.

***Index******terms:***Hybrid Quantum-Classical Systems, Gaussian boson sampling, Variational Quantum Eigensolver, Rabi Fit, Fidelity, EMD.

1. **INTRODUCTION**

conventional carry select adder performs better in terms of speed. The delay of our proposed design increases lightly because of logic circuit sharing sacrifices the length of parallel path.


However, the proposed area-efficient carry select adder retains partial parallel computation architecture as the conventional carry select adder

to excess-1 code converters (BEC) to improve the speed of addition. This logic can be implemented with any type of adder to further improve the speed. Using Binary to Excess-1 Converter (BEC) instead of RCA in the regular CSLA we can achieve lower area and power consumption. The main advantage of this BEC logic comes from the lesser number of logic gates than the Full Adder (FA) structure.the basic idea of the proposed work is by using n-bit binary to excess-1 code converters (BEC) to improve the speed of addition. This logic can be implemented with any type of adder to further improve the speed. Using Binary to Excess-1 Converter (BEC) instead of RCA in the regular CSLA we can achieve lower area and power consumption. The main advantage of this BEC logic comes from the lesser number of logic gates than the Full Adder (FA) structure.

1. **DELAY AND AREA EVALUATION OF THE BASIC ADDER BLOCKS**

Binary to excess-1 code converters (BEC) to improve the speed of addition. This logic can be implemented with any type of adder to further improve the speed. Using Binary to Excess-1 Converter (BEC) instead of RCA in the regular CSLA we can achieve lower area and power consumption. The main advantage of this BEC logic comes from the lesser number of logic gates than the Full Adder (FA) structure.and area equal to 1 unit. We then add up the number of gates in the longest path of a logic block that contributes to the maximum delay. The area evaluation is done by counting the total number of AOI gates required for each logic block.

Based on this approach, the CSLA adder blocks of 2:1 mux, Half Adder (HA), and FA are evaluated and listed in Table I.



**Figure 1: Delay and Area evaluation of an XOR gate**.

Table 1

Delay and Area Evaluation of the Basic Blocks of CSLA

Basic Blocks Delay Area

XOR 3 5

2:1 MUX 3 4


Half Adder 3 6

Full Adder 6 13

1. **BASIC STRUCTURE OF BEC LOGIC**

conventional carry select adder performs better in terms of speed. The delay of our proposed design increases lightly because of logic circuit sharing sacrifices the length of parallel path.

However, the proposed area-efficient carry select adder retains partial parallel computation architecture as the conventional carry select adder area and power consumption of the regular CSLA. To replace the n-bit RCA, an n+1-bit BEC is required. A structure and the function table of a 4-bit BEC are shown in Figure.2 and Table .2, respectively.



**Figure 2: 4-Bit BEC**

The Boolean expressions of the 4-bit BEC are


X0 = ~B0 (1)

X1 = B0^B1 (2)


X2 = B2^ (B0 & B1) (3)

X3 = B3^ (B0 & B1 & B2) (4)

**Table.2 Function table of the 4-bit BEC**



1. **BASIC STRUCTURE OF REGULAR 16-BIT CSLA**



**Figure 3: Regular CSLA circuit**

The structure of the 16-b regular SQRT CS conventional carry select adder performs better in terms of speed. The delay of our proposed design increases lightly because of logic circuit sharing sacrifices the length of parallel path.

However, the proposed area-efficient carry select adder retains partial parallel computation architecture as the conventional carry select adder

{c6, sum [6:4]} = c3 [t=10] +mux (5)

{c10, sum [10:7]} = c6 [t=13] +mux (6)

{Cout, sum [15:11]}=c10 [t=16] +mux. (7)

3) The one set of 2-b RCA in group2 has 2 FA for Cin=1 and the other set has 1 FA and 1 HA for Cin=0. Based on the area count of Table I, the total number of gate counts in group2 is determined as follows:

Gate Count = 57 (FA+HA+MUX) (8)

FA=39(3\*13) (9)

HA=6(1\*6) (10)

MUX=12(3\*4) (11)

4) Similarly, the estimated maximum delay and area of the other groups in the regular SQRT CSLA are evaluated and listed in Table 3.

Table 3

Group Delay Area

2 11 57

3 13 87

4 16 117


5 19 147

1. **DELAY AND AREA EVALUATION OF CSLA USING BEC CONVERTER**

.

The structure of the proposed 16-b SQRT CSLA using BEC for RCA with Cin=1 to optimize the area and power is shown in Fig. 4. We again split the structure into five groups. The steps leading to the conventional carry select adder performs better in terms of speed. The delay of our proposed design increases lightly because of logic circuit sharing sacrifices the length of parallel path

However, the proposed area-efficient carry select adder retains partial parallel computation architecture as the conventional carry select adder) are depending on s3and mux and partial c3 (input to mux) and mux, respectively. The sum2 depends on c1 and mux.

2) For the remaining group’s the arrival time of mux selection input is always greater than the arrival time of data inputs from the BEC’s. Thus, the delay of the remaining groups depends on the arrival time of mux selection input and the mux delay.

3) The area count of group2 is determined as follows:

Gate count =43(FA+HA+MUX+BEC) (12)

FA= 13(1\*13) (13)

HA=6(1\*6) (14)

AND=NOT=1 (15)

XOR=10(2\*5) (16)

MUX=12(3\*4) (17)

4) Similarly, the estimated maximum delay and area of the other groups of the modified SQRT CSLA are evaluated and listed in Table 4.

Table 4

Group Delay Area


2 13 43

3 16 61

4 19 84

5 22 107

Comparing Tables 3and 4, it is clear that the proposed modified CSLA saves 113 gate areas than the regular CSLA, with only 11 increases in gate delays.



**Figure 4: CSLA circuit using BEC Converter**

1. **SIMULATIONS AND EXPERIMENTAL RESULTS**

The proposed solutions have been designed using Xilinx. The area-efficient carry select adder can also achieve an outstanding performance in power consumption. Power consumption can be greatly saved in our proposed area-efficient carry select adder because we only need one XOR gate and one INV gate in each summation operation as well as one AND gate and one OR gate in each carry-out operation after logic simplification and sharing partial circuit. Because of hardware sharing, we can also significantly reduce the occurring chance of glitch. Besides, the improvement of power consumption can be more obvious as the input bit number increases.

**Figure 5: Simulated Results**

The conventional carry select adder performs better in terms of speed. The delay of our proposed design increases lightly because of logic circuit sharing sacrifices the length of parallel path.

However, the proposed area-efficient carry select adder retains partial parallel computation architecture as the conventional carry select adder design; the delay increment of the proposed design is similar to that in the conventional design as the input bit number increases. We also simulated the delay performance in the proposed area-efficient adder and conventional carry select adder with 4, 8, 16, and 32-bit respectively.

**CONCLUSION**

Implemented with any type of adder to further improve the speed. Using Binary to Excess-1 Converter (BEC) instead of RCA in the regular CSLA we can achieve lower area and power consumption. The main advantage of this BEC logic comes from the lesser number of logic gates than the Full Adder (FA) structure.is therefore, low area, low power, simple and efficient A to excess-1 code converters (BEC) to improve the speed of addition. This logic can be for VLSI hardware implementation.

**REFERENCES**

[1] O. J. Bedrij, “Carry-select adder,” *IRE Trans. Electron. Comput,* pp. 340–344, 1962.

[2] B. Ramkumar, H.M. Kittur, and P. M. Kannan, “ASIC implementation of modified faster carry save adder,” *Eur. J. Sci. Res.*, vol. 42, no. 1, pp.53–58, 2010.

[3] T. Y. Ceiang and M. J. Hsiao, “Carry-select adder using single ripple carry adder,” *Electron. Lett.*, vol. 34, no. 22, pp. 2101–2103, Oct. 1998.

[4] J. M. Rabaey*, Digtal Integrated Circuits— A Design Perspective* Upper Saddle River, NJ: Prentice-Hall, 2001

[5] J. M. Rabaey*, Digtal Integrated Circuits— A Design Perspective* Upper Saddle River, NJ: Prentice-Hall, 2001.

[6] Y. He, C. H. Chang, and J. Gu, “An area efficient 64-bit square root carry-select adder for lowpower applications,” in *Proc. IEEE Int. Symp. Circuits Syst.*, 2005, vol. 4, pp. 4082–4085.

[7] Cadence, “Encounter user guide,” Version 6.2.4, March 2008

★★★